# MINEOLA WATER UTILITIES

MONTHLY ACTIVITY REPORT

**MONTH OF: October, 2018**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 124 Hrs.

Customer Water Connections.............................................................. 32

Customer Water Disconnections.......................................................... 40

Turn water off for leak ................................. 05

Reread .................................................... 05

Water Leaks Reported.......................................................................... 14 . Paid turn water back on 09

Locate Water Lines for Others............................................................. 01

O & M Water Production & Distribution System (hours)................... 372 hrs.

Miscellaneous ........................................................................... 23

Pulled meter logs ........................................................................... 05

Number of water Meters Read..............................................................2,701

Number of active accounts............................................................ 2,430 29 city acct.

Disconnects for Non-Payment.............................................................. 25

Change meter register -------------------------------------------------------- 0

Repairs complete turn water on---------------------------------------------- 4

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 14.008 M.G.

Average Usage per Day................................................................... .. 0.451 M.G

Highest Usage per Day...................................................................... . 0.539 M.G.

Pounds of Disinfectant Used................................................................. 461 lbs.

Average Pounds of Disinfectant Used per Day.................................... 14.8 lbs.

Pounds. Of Sequestering Agent Used................................................. 127 .00 lbs. Average Pounds of Sequestering agent used per Day...................... 4.1 lbs.

Pounds of Fluoride Used....................................................................... 213 lbs.

Average pounds of Fluoride Used ............................................. 6.8 lbs.

# MINEOLA WATER UTILITY

**MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................15

Customer Stoppages................................................................ 11

Lift Station Inspections Performed.......................................... 062 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 372 hrs.

Number of Feet of sewer Main cleared.............................. 2,250 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 093 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 11/05/2018