#  MINEOLA WATER UTILITIES

 MONTHLY ACTIVITY REPORT

**MONTH OF: February, 2019**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 112 Hrs.

Customer Water Connections.............................................................. 46

Customer Water Disconnections.......................................................... 42

Turn water off for leak ................................. 09

Reread .................................................... 08

Water Leaks Reported.......................................................................... 16 . Paid turn water back on 13

Locate Water Lines for Others............................................................. 02

O & M Water Production & Distribution System (hours)................... 336 hrs.

Miscellaneous ........................................................................... 14

Pulled meter logs ........................................................................... 06

Number of water Meters Read..............................................................2,701

 Number of active accounts............................................................ 2,421 29 city acct.

Disconnects for Non-Payment.............................................................. 30

Change meter register -------------------------------------------------------- 02

Repairs complete turn water on---------------------------------------------- 02

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 11.249 M.G.

Average Usage per Day................................................................... .. 0.401 M.G

Highest Usage per Day...................................................................... . 0.516 M.G.

 Pounds of Disinfectant Used................................................................. 388 lbs.

 Average Pounds of Disinfectant Used per Day.................................... 13.8 lbs.

Pounds. Of Sequestering Agent Used................................................. 82 .60 lbs. Average Pounds of Sequestering agent used per Day...................... 2.9 lbs.

Pounds of Fluoride Used....................................................................... 137 lbs.

Average pounds of Fluoride Used ............................................. 4.9 lbs.

#  MINEOLA WATER UTILITY

 **MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................15

Lift Station Inspections Performed.......................................... 112 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 336 hrs.

Number of Feet of sewer Main cleared.............................. 1,500 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

 Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 084 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 03/04/2019