#  MINEOLA WATER UTILITIES

 MONTHLY ACTIVITY REPORT

**MONTH OF: August, 2019**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 124 Hrs.

Customer Water Connections.............................................................. 42

Customer Water Disconnections.......................................................... 44

Turn water off for leak ................................. 11

Reread .................................................... 04

Water Leaks Reported.......................................................................... 12 . Paid turn water back on 08

Locate Water Lines for Others............................................................. 02

O & M Water Production & Distribution System (hours)................... 496 hrs.

Miscellaneous ........................................................................... 01

Pulled meter logs ........................................................................... 01

Number of water Meters Read..............................................................2,708

 Number of active accounts............................................................ 2,452 29 city acct.

Disconnects for Non-Payment.............................................................. 22

Change meter register -------------------------------------------------------- 04

Set Meter -------------------------------------------------------------------------- 00

Repairs complete turn water on---------------------------------------------- 01

Lock Meters--------------------------------------------------------------------- 05

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 20.150 M.G.

Average Usage per Day................................................................... .. 0.650 M.G

Highest Usage per Day...................................................................... . 0.927 M.G.

 Pounds of Disinfectant Used................................................................. 748 lbs.

 Average Pounds of Disinfectant Used per Day.................................... 24.1 lbs.

Pounds. Of Sequestering Agent Used................................................. 186 .44 lbs. Average Pounds of Sequestering agent used per Day...................... 6.0 lbs.

Pounds of Fluoride Used....................................................................... 246 lbs.

Average pounds of Fluoride Used ............................................. 7.9 lbs.

#  MINEOLA WATER UTILITY

 **MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................06

Lift Station Inspections Performed.......................................... 120 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 496 hrs.

Number of Feet of sewer Main cleared.............................. 900 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

 Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 124 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 09/04/2019