# MINEOLA WATER UTILITIES

MONTHLY ACTIVITY REPORT

**MONTH OF: October, 2019**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 124 Hrs.

Customer Water Connections.............................................................. 37

Customer Water Disconnections.......................................................... 30

Turn water off for leak ................................. 07

Reread .................................................... 07

Water Leaks Reported.......................................................................... 22 . Paid turn water back on 17

Locate Water Lines for Others............................................................. 05

O & M Water Production & Distribution System (hours)................... 496 hrs.

Miscellaneous ........................................................................... 15

Pulled meter logs ........................................................................... 07

Number of water Meters Read..............................................................2,713

Number of active accounts............................................................ 2,450 29 city acct.

Disconnects for Non-Payment.............................................................. 41

Change meter register -------------------------------------------------------- 04

Set Meter -------------------------------------------------------------------------- 03

Repairs complete turn water on---------------------------------------------- 01

Lock Meters--------------------------------------------------------------------- 06

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 15.750 M.G.

Average Usage per Day................................................................... .. 0.508 M.G

Highest Usage per Day...................................................................... . 0.677 M.G.

Pounds of Disinfectant Used................................................................. 580 lbs.

Average Pounds of Disinfectant Used per Day.................................... 19.0 lbs.

Pounds. Of Sequestering Agent Used................................................. 136 .88 lbs. Average Pounds of Sequestering agent used per Day...................... 4.4 lbs.

Pounds of Fluoride Used....................................................................... 197 lbs.

Average pounds of Fluoride Used ............................................. 6.3 lbs.

# MINEOLA WATER UTILITY

**MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................13

Lift Station Inspections Performed.......................................... 062 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 496 hrs.

Number of Feet of sewer Main cleared.............................. 1,300 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 124 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 11/06/2019