# MINEOLA WATER UTILITIES

MONTHLY ACTIVITY REPORT

**MONTH OF: November, 2019**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 120 Hrs.

Customer Water Connections.............................................................. 21

Customer Water Disconnections.......................................................... 28

Turn water off for leak ................................. 05

Reread .................................................... 03

Water Leaks Reported.......................................................................... 25 . Paid turn water back on 02

Locate Water Lines for Others............................................................. 03

O & M Water Production & Distribution System (hours)................... 480 hrs.

Miscellaneous ........................................................................... 19

Pulled meter logs ........................................................................... 02

Number of water Meters Read..............................................................2,713

Number of active accounts............................................................ 2,460 29 city acct.

Disconnects for Non-Payment.............................................................. 25

Change meter register -------------------------------------------------------- 03

Set Meter -------------------------------------------------------------------------- 02

Repairs complete turn water on---------------------------------------------- 02

Lock Meters--------------------------------------------------------------------- 03

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 13.528 M.G.

Average Usage per Day................................................................... .. 0.450 M.G

Highest Usage per Day...................................................................... . 0.537 M.G.

Pounds of Disinfectant Used................................................................. 482 lbs.

Average Pounds of Disinfectant Used per Day.................................... 16.0 lbs.

Pounds. Of Sequestering Agent Used................................................. 108 .00 lbs. Average Pounds of Sequestering agent used per Day...................... 3.6 lbs.

Pounds of Fluoride Used....................................................................... 128 lbs.

Average pounds of Fluoride Used ............................................. 4.2 lbs.

# MINEOLA WATER UTILITY

**MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................12

Lift Station Inspections Performed.......................................... 060 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 480 hrs.

Number of Feet of sewer Main cleared.............................. 1,800 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 120 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 12/09/2019