#  MINEOLA WATER UTILITIES

 MONTHLY ACTIVITY REPORT

**MONTH OF: June, 2020**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 120 Hrs.

Customer Water Connections.............................................................. 33

Customer Water Disconnections.......................................................... 30

Turn water off for leak ................................. 07

Reread .................................................... 02

Water Leaks Reported.......................................................................... 08 . Paid turn water back on 00

Locate Water Lines for Others............................................................. 03

O & M Water Production & Distribution System (hours)................... 480 hrs.

Miscellaneous ........................................................................... 06

Pulled meter logs ........................................................................... 01

Number of water Meters Read..............................................................2,708

 Number of active accounts............................................................ 2,460 29 city acct.

Disconnects for Non-Payment.............................................................. 00

Change meter register -------------------------------------------------------- 02

Set Meter -------------------------------------------------------------------------- 01

Repairs complete turn water on---------------------------------------------- 01

Lock Meters--------------------------------------------------------------------- 01

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 13.626 M.G.

Average Usage per Day................................................................... .. 0.454 M.G

Highest Usage per Day...................................................................... . 0.593 M.G.

 Pounds of Disinfectant Used................................................................. 636 lbs.

 Average Pounds of Disinfectant Used per Day.................................... 21.0 lbs.

Pounds. Of Sequestering Agent Used................................................. 158 .00 lbs. Average Pounds of Sequestering agent used per Day...................... 5.2 lbs.

Pounds of Fluoride Used....................................................................... 192 lbs.

Average pounds of Fluoride Used ............................................. 6.0 lbs.

#  MINEOLA WATER UTILITY

 **MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................04

Lift Station Inspections Performed.......................................... 060 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 480 hrs.

Number of Feet of sewer Main cleared.............................. 600 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

 Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 120 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 7/02/2020