#  MINEOLA WATER UTILITIES

 MONTHLY ACTIVITY REPORT

**MONTH OF: September, 2020**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 120 Hrs.

Customer Water Connections.............................................................. 32

Customer Water Disconnections.......................................................... 39

Turn water off for leak ................................. 07

Reread .................................................... 01

Water Leaks Reported.......................................................................... 09 . Paid turn water back on 09

Locate Water Lines for Others............................................................. 01

O & M Water Production & Distribution System (hours)................... 480 hrs.

Miscellaneous ........................................................................... 12

Pulled meter logs ........................................................................... 06

Number of water Meters Read..............................................................2,710

 Number of active accounts............................................................ 2,457 29 city acct.

Disconnects for Non-Payment.............................................................. 30

Change meter register -------------------------------------------------------- 03

Set Meter -------------------------------------------------------------------------- 00

Repairs complete turn water on---------------------------------------------- 01

Lock Meters--------------------------------------------------------------------- 04

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 15.787 M.G.

Average Usage per Day................................................................... .. 0.526 M.G

Highest Usage per Day...................................................................... . 0.693 M.G.

 Pounds of Disinfectant Used................................................................. 490 lbs.

 Average Pounds of Disinfectant Used per Day.................................... 16.3 lbs.

Pounds. Of Sequestering Agent Used................................................. 141 .00 lbs. Average Pounds of Sequestering agent used per Day...................... 4.7 lbs.

Pounds of Fluoride Used....................................................................... 219 lbs.

Average pounds of Fluoride Used ............................................. 7.3 lbs.

#  MINEOLA WATER UTILITY

 **MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................06

Lift Station Inspections Performed.......................................... 060 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 360 hrs.

Number of Feet of sewer Main cleared.............................. 900 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

 Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 120 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 10/08/2020