# MINEOLA WATER UTILITIES

MONTHLY ACTIVITY REPORT

**MONTH OF: March, 2021**

**WATER:**

Bacteriological Analysis...................................................................... 06

Pump Station Inspections.................................................................... 124 Hrs.

Customer Water Connections.............................................................. 40

Customer Water Disconnections.......................................................... 36

Turn water off for leak ................................. 09

Reread .................................................... 11

Water Leaks Reported.......................................................................... 11 . Paid turn water back on 09

Locate Water Lines for Others............................................................. 03

O & M Water Production & Distribution System (hours)................... 496 hrs.

Miscellaneous ........................................................................... 23

Pulled meter logs ........................................................................... 17

Number of water Meters Read..............................................................2,717

Number of active accounts............................................................ 2,468 29 city acct.

Disconnects for Non-Payment.............................................................. 24

Change meter register -------------------------------------------------------- 11

Set Meter -------------------------------------------------------------------------- 01

Repairs complete turn water on---------------------------------------------- 11

Lock Meters--------------------------------------------------------------------- 01

**PRODUCTION & TREATMENT**

Water Produced in Million Gallons........................................... 15.172 M.G.

Average Usage per Day................................................................... .. 0.489 M.G

Highest Usage per Day...................................................................... . 0.583 M.G.

Pounds of Disinfectant Used................................................................. 477 lbs.

Average Pounds of Disinfectant Used per Day.................................... 15.0 lbs.

Pounds. Of Sequestering Agent Used................................................. 101 .00 lbs. Average Pounds of Sequestering agent used per Day...................... 3.2 lbs.

Pounds of Fluoride Used....................................................................... 127 lbs.

Average pounds of Fluoride Used ............................................. 4.0 lbs.

# MINEOLA WATER UTILITY

**MONTHLY ACTIVITY REPORT**

**WASTEWATER:**

Sewer Stoppages Reported......................................................19

Lift Station Inspections Performed.......................................... 124 hrs.

Sewer Taps Installed ----------------------------------------------- 0

O & M of Wastewater Collection System (hours)................... 496 hrs.

Number of Feet of sewer Main cleared.............................. 2,850 ft.

**UTILITY MAINTENANCE:**

Vehicle Maintenance......checked daily

Older trucks check for mechanical problems and returned to service.

Equipment Maintenance........................................................ 124 hrs. EST.

Submitted by: Rolando Ortega

Water: Dept Date: 4/09/2021