**Month of: November, 2021**

|  |  |
| --- | --- |
| WATER: |  |
| Bacteriological Analysis | 06 |
| Pump Station Inspections | 120 Hrs. |
| Customer Water Connections | 37 |
| Customer Water Disconnections | 34 |
| Turn water off for leak | 04 |
| Reread | 00 |
| Water Leaks Reported | 14 |
| Paid turn water back on  | 05 |
| Locate Water Lines for Others | 01 |
| O&M Water Production & Distribution System (hours) | 480 hrs. |
| Miscellaneous | 15 |
| Pulled Meter Logs | 00 |
| Number of Water Meters Read | 2,756 |
| Number of Active Accounts (29 city acct.) | 2,487 |
| Disconnects for Non-Payment | 20 |
| Change Meter register | 14 |
| Set Meter | 02 |
| Repairs complete turn water on | 01 |
| Lock Meters | 07 |
| Leak at Meter | 06 |
| PRODUCTION & TREATMENT: |  |
| Water Produced in Million Gallons | 13.463 M.G. |
| Average Usage per Day | 0.448 M.G. |
| Highest Usage per Day | 0.600 M.G. |
| Pounds of Disinfectant Used | 500 lbs. |
| Average Pounds of Disinfectant Used per Day | 16.0 lbs. |
| Pounds of Sequestering Agent Used | 127.00 lbs. |
| Average Pounds of Sequestering agent used per Day | 4.2 lbs. |
| Pounds of Fluoride Used | 173 lbs. |
| WASTEWATER: |  |
| Sewer Stoppages Reported | 06 |
| Lift Station Inspections Performed | 060 Hrs. |
| Sewer Taps Installed | 1 |
| O&M of Wastewater Collection System (hours) | 480 Hrs. |
| Number of Feet of Sewer Main Cleared | 900 ft.  |
|  |  |
| UTILITY MAINTENANCE: |  |
| Vehicle Maintenance | Checked Daily |
| Older trucks check for mechanical problems and returned to service |  |
| Equipment Maintenance | 120 hrs. EST. |

Submitted by: Rolando Ortega