**Month of: July, 2022**

|  |  |
| --- | --- |
| WATER: |  |
| Bacteriological Analysis | 06 |
| Pump Station Inspections | 124 Hrs. |
| Customer Water Connections | 41 |
| Customer Water Disconnections | 33 |
| Turn water off for leak | 07 |
| Reread | 07 |
| Water Leaks Reported | 09 |
| Paid turn water back on | 07 |
| Locate Water Lines for Others | 04 |
| O&M Water Production & Distribution System (hours) | 496 hrs. |
| Miscellaneous | 33 |
| Pulled Meter Logs | 02 |
| Number of Water Meters Read | 2,815 |
| Number of Active Accounts (29 city acct.) | 2,531 |
| Disconnects for Non-Payment | 25 |
| Change Meter register (Dead Batteries). | 11 |
| Set Meter | 02 |
| Repairs complete turn water on | 02 |
| Lock Meters | 05 |
| Leak at Meter | 00 |
| PRODUCTION & TREATMENT: |  |
| Water Produced in Million Gallons | 22.443 M.G. |
| Average Usage per Day | 0.723 M.G. |
| Highest Usage per Day | 1.854 M.G. |
| Pounds of Disinfectant Used | 775 lbs. |
| Average Pounds of Disinfectant Used per Day | 25.0 lbs. |
| Pounds of Sequestering Agent Used | 207.00 lbs. |
| Average Pounds of Sequestering agent used per Day | 6.7 lbs. |
| Pounds of Fluoride Used | 310 lbs. |
| WASTEWATER: |  |
| Sewer Stoppages Reported | 05 |
| Lift Station Inspections Performed | 124 Hrs. |
| Sewer Taps Installed | 0 |
| O&M of Wastewater Collection System (hours) | 496 Hrs. |
| Number of Feet of Sewer Main Cleared | 0,750 ft. |
|  |  |
| UTILITY MAINTENANCE: |  |
| Vehicle Maintenance | Checked Daily |
| Older trucks check for mechanical problems and returned to service |  |
| Equipment Maintenance | 124 Hrs. EST. |

Submitted by: Rolando Ortega